IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
File name: "Project Number"
Time stamp: "2019-08-26T14:07:48"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20150220_1215(x64) - Exporter 16.0.428.0 - Default UI"
Application: "Autodesk Revit 2016 (ENU)" version "2016" identifier "Revit" by Organization "Autodesk Revit 2016 (ENU)"

People and organizations
  Person "ksubramanya" of Organization (no name given)
  Owner history of Person "ksubramanya" of Organization (no name given) | application "Autodesk Revit 2016 (ENU)" version "2016" identifier "Revit" by Organization "Autodesk Revit 2016 (ENU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  PRESSUREUNIT: PASCAL

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 51° 30′ 23.112487″ | longitude -0° 7′ 37.956022″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "London", "London", "United Kingdom"
      IFCBUILDINGSTOREY "Level 0" | long name "Level 0" | elevation 0.
        contains 5 elements
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "std(nested)" | object type "std(nested)" | names: "ZZZ_do_not_use_PIF_UN_Gully bodies_Without lateral inlet_ACO:std(nested):294684" | material: "Plastic,Black" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Constraints, Dimensions, General, Identity Data
          1 x IFCFLOWTERMINAL | type IFCWASTETERMINALTYPE "std(nested)" | object type "std(nested)" | names: "ZZZ_do_not_use_PF_UN_foul air trap_ACO:std(nested):294685" | material: "Plastic,Black" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Constraints, Dimensions, General, Identity Data
          1 x IFCFLOWTERMINAL | type IFCWASTETERMINALTYPE "std(nested)" | object type "std(nested)" | names: "ZZZ_do_not_use_PF_UN_compressed seal flange_ACO:std(nested):294686" | material: "Plastic, Grey" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Constraints, Dimensions, General, Identity Data
          1 x IFCFLOWCONTROLLER | type IFCDAMPERTYPE "std(nested)" | object type "std(nested)" | names: "ZZZ_do_not_use_PF_UN_Fit-in installation set_ACO:std(nested):294687" | material: "Concrete, Lightweight, 45" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Constraints, Dimensions, General, Identity Data
          1 x IFCFLOWTERMINAL | type IFCWASTETERMINALTYPE "std(nested)" | object type "std(nested)" | names: "ZZZ_do_not_use_PIF_UN_Fire protection set_ACO:std(nested):294688" | material: "Plastic,Black" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Constraints, Dimensions, General, Identity Data

Types
  IFCPIPEFITTINGTYPE "std(nested)" | USERDEFINED | 1 occurrence | material: "Plastic,Black" | property sets: Constraints, Dimensions, General, Identity Data, Materials and Finishes, Other | description "ACO Gully body"
  IFCWASTETERMINALTYPE "std(nested)" | FLOORTRAP | 1 occurrence | material: "Plastic,Black" | property sets: General, Identity Data, Other | description "ACO Foul air trap"
  IFCWASTETERMINALTYPE "std(nested)" | FLOORTRAP | 1 occurrence | material: "Plastic, Grey" | property sets: Dimensions, General, Identity Data, Other | description "ACO Compressed seal flange"
  IFCDAMPERTYPE "std(nested)" | FIREDAMPER | 1 occurrence | material: "Concrete, Lightweight, 45" | property sets: General, Identity Data, Materials and Finishes, Other | description "ACO fit-in installation set"
  IFCWASTETERMINALTYPE "std(nested)" | FLOORTRAP | 1 occurrence | material: "Plastic,Black" | property sets: General, Identity Data, Other | description "ACO Fire protection set"

Property sets
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "Project Number" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Other | properties | on 1 object (1 IFCFLOWFITTING)
    Category = "Pipe Fittings" (IFCLABEL)
    Family = "ZZZ_do_not_use_PIF_UN_Gully bodies_Without lateral inlet_ACO: std(nested)" (IFCLABEL)
    Family and Type = "ZZZ_do_not_use_PIF_UN_Gully bodies_Without lateral inlet_ACO: std(nested)" (IFCLABEL)
    Fire protection = TRUE (IFCBOOLEAN)
    Fit in installation = TRUE (IFCBOOLEAN)
    RSen_C_width = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_width_01 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_width_02 = 149. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_width_03 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Recess = "200x200" (IFCTEXT)
    Schedule Level = "Level: Level 0" (IFCLABEL)
    Type = "ZZZ_do_not_use_PIF_UN_Gully bodies_Without lateral inlet_ACO: std(nested)" (IFCLABEL)
    Type Id = "ZZZ_do_not_use_PIF_UN_Gully bodies_Without lateral inlet_ACO: std(nested)" (IFCLABEL)
    Visibility_Vertical = TRUE (IFCBOOLEAN)
    product_index = 3 (IFCINTEGER)
    type_index = 3 (IFCINTEGER)
    type_index1 = 3 (IFCINTEGER)
    visibility_side = FALSE (IFCBOOLEAN)
  Other | properties | on 1 object (1 IFCFLOWTERMINAL)
    Category = "Plumbing Fixtures" (IFCLABEL)
    Family = "ZZZ_do_not_use_PF_UN_foul air trap_ACO: std(nested)" (IFCLABEL)
    Family and Type = "ZZZ_do_not_use_PF_UN_foul air trap_ACO: std(nested)" (IFCLABEL)
    Type = "ZZZ_do_not_use_PF_UN_foul air trap_ACO: std(nested)" (IFCLABEL)
    Type Id = "ZZZ_do_not_use_PF_UN_foul air trap_ACO: std(nested)" (IFCLABEL)
    type_index = 3 (IFCINTEGER)
  Other | properties | on 1 object (1 IFCFLOWTERMINAL)
    Category = "Plumbing Fixtures" (IFCLABEL)
    Family = "ZZZ_do_not_use_PF_UN_compressed seal flange_ACO: std(nested)" (IFCLABEL)
    Family and Type = "ZZZ_do_not_use_PF_UN_compressed seal flange_ACO: std(nested)" (IFCLABEL)
    Type = "ZZZ_do_not_use_PF_UN_compressed seal flange_ACO: std(nested)" (IFCLABEL)
    Type Id = "ZZZ_do_not_use_PF_UN_compressed seal flange_ACO: std(nested)" (IFCLABEL)
  Other | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Category = "Plumbing Fixtures" (IFCLABEL)
    Family = "ZZZ_do_not_use_PF_UN_Fit-in installation set_ACO: std(nested)" (IFCLABEL)
    Family and Type = "ZZZ_do_not_use_PF_UN_Fit-in installation set_ACO: std(nested)" (IFCLABEL)
    Type = "ZZZ_do_not_use_PF_UN_Fit-in installation set_ACO: std(nested)" (IFCLABEL)
    Type Id = "ZZZ_do_not_use_PF_UN_Fit-in installation set_ACO: std(nested)" (IFCLABEL)
  Other | properties | on 1 object (1 IFCFLOWTERMINAL)
    Category = "Plumbing Fixtures" (IFCLABEL)
    Family = "ZZZ_do_not_use_PIF_UN_Fire protection set_ACO: std(nested)" (IFCLABEL)
    Family and Type = "ZZZ_do_not_use_PIF_UN_Fire protection set_ACO: std(nested)" (IFCLABEL)
    Type = "ZZZ_do_not_use_PIF_UN_Fire protection set_ACO: std(nested)" (IFCLABEL)
    Type Id = "ZZZ_do_not_use_PIF_UN_Fire protection set_ACO: std(nested)" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Circle Head - Project Datum" (IFCLABEL)
    Family and Type = "Level: Circle Head - Project Datum" (IFCLABEL)
    Type = "Level: Circle Head - Project Datum" (IFCLABEL)
    Type Id = "Level: Circle Head - Project Datum" (IFCLABEL)
  Other: 5 more contents on 0 objects not shown
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Circle Head - Project Datum" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCFLOWFITTING)
    Mark = "1" (IFCTEXT)
    RSen_C_code_article = "2500.55.00" (IFCTEXT)
    RSen_C_code_gtin = "4002626128386" (IFCTEXT)
    RSen_C_description = "ACO Easy-Flow Bodenablauf DN50/ 90 Grad/ 1,5/s/ Kst Halter./ WS50" (IFCTEXT)
    RSen_C_type_comments = "" (IFCTEXT)
    Version = "Standard" (IFCTEXT)
    productrange = "Easyflow" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCFLOWTERMINAL)
    Mark = "1" (IFCTEXT)
    RSen_C_code_article = "2520.00.00" (IFCTEXT)
    RSen_C_code_gtin = "Not available" (IFCTEXT)
    RSen_C_description = "ACO Easy-Flow Brandschutzset DN50/90 Grad/ zu Ablaufkörper" (IFCTEXT)
    RSen_C_type_comments = "" (IFCTEXT)
    productrange = "Easyflow" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCFLOWTERMINAL)
    Mark = "2" (IFCTEXT)
    RSen_C_code_article = "2040.00.02" (IFCTEXT)
    RSen_C_code_gtin = "Not available" (IFCTEXT)
    RSen_C_description = "ACO Easy-Flow Pressdichtungsfl Halter./ für Punktentw" (IFCTEXT)
    productrange = "Easyflow" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Mark = "3" (IFCTEXT)
    RSen_C_code_article = "9390.08.40" (IFCTEXT)
    RSen_C_code_gtin = "not available" (IFCTEXT)
    RSen_C_description = "ACO Fit-In Einbauset Easy-Flow DN50/ 90 Grad/ A1" (IFCTEXT)
    productrange = "Easyflow" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCFLOWTERMINAL)
    Mark = "4" (IFCTEXT)
    RSen_C_code_article = "Not available" (IFCTEXT)
    RSen_C_code_gtin = "Not available" (IFCTEXT)
    RSen_C_description = "ACO Brandschutzset Dia.43" (IFCTEXT)
    productrange = "Easyflow" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 0" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data: 5 more contents on 0 objects not shown
  Pset_ManufacturerTypeInformation | properties | on 5 objects (3 IFCFLOWTERMINAL, 1 IFCFLOWCONTROLLER, 1 IFCFLOWFITTING)
    Manufacturer = "ACO" (IFCLABEL)
  Pset_DistributionFlowElementCommon | properties | on 5 objects (3 IFCFLOWTERMINAL, 1 IFCFLOWCONTROLLER, 1 IFCFLOWFITTING)
    Reference = "std(nested)" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCFLOWFITTING)
    Level = "Level: Level 0" (IFCLABEL)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_height = 114. (IFCLENGTHMEASURE) [MILLI METRE]
    Work Plane = "Level : Level 0" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCFLOWTERMINAL)
    Host = "None" (IFCTEXT)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = -150.00000000003 (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCFLOWTERMINAL)
    Host = "None" (IFCTEXT)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = -138.000000000031 (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Host = "None" (IFCTEXT)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = -282.88236382739 (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCFLOWTERMINAL)
    Host = "None" (IFCTEXT)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = -252.000000000001 (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 type object
    Default Elevation = 1219.2 (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCFLOWFITTING)
    Area = 0.0604335008951904 (IFCAREAMEASURE) [SQUARE_METRE]
    RSen_C_diameter = 149. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_diameter_01 = 125. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_diameter_02 = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_diameter_03 = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_height_03 = 53. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_height_04 = 12. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_height_05 = 138. (IFCLENGTHMEASURE) [MILLI METRE]
    Size = "" (IFCTEXT)
    Volume = 0.00210771227696554 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCFLOWTERMINAL)
    Area = 0.0223850059280305 (IFCAREAMEASURE) [SQUARE_METRE]
    D1 = 93. (IFCLENGTHMEASURE) [MILLI METRE]
    H1 = 92. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.000240709648233896 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCFLOWTERMINAL)
    Area = 0.0608659892475411 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.000176491795758041 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Area = 0.10610719718982 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.0032882409482898 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCFLOWTERMINAL)
    Area = 0.00838151003480693 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 3.05002753565898E-5 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    RSen_P_c01_angle = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Dimensions | properties | on 1 type object
    RSen_C_diameter = 303. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_diameter_01 = 130. (IFCLENGTHMEASURE) [MILLI METRE]
  General | properties | on 1 object (1 IFCFLOWFITTING)
    RSen_S_net_mass = 0.5 (IFCREAL)
  General | properties | on 1 object (1 IFCFLOWTERMINAL)
    RSen_S_net_mass = 0.1 (IFCREAL)
  General | properties | on 1 object (1 IFCFLOWTERMINAL)
    RSen_S_net_mass = 0.6 (IFCREAL)
  General | properties | on 1 object (1 IFCFLOWCONTROLLER)
    RSen_S_net_mass = 3.1 (IFCREAL)
  General | properties | on 1 object (1 IFCFLOWTERMINAL)
    RSen_C_intended_use = "Entwässerungssysteme" (IFCTEXT)
    RSen_S_net_mass = 0.2 (IFCREAL)
  General | properties | on 1 type object
    RSen_C_code_ETIM = "EC010284" (IFCTEXT)
    RSen_C_code_manufacturer_gln = "4399901709010" (IFCTEXT)
    RSen_C_code_specification_URL = "" (IFCTEXT)
    RSen_C_content_creator = "ACO Technology Centre Private Limited" (IFCTEXT)
    RSen_C_content_date_changed = "" (IFCTEXT)
    RSen_C_content_version = "1.0" (IFCTEXT)
    RSen_C_info_commercial = "http://catalogue.aco-buildingdrainage.com/Home/Products/Collect/Bathroom-drainage/Bathroom-gullies/Easyflow/Gully-bodies-DN-50" (IFCTEXT)
    RSen_C_info_technical = "http://catalogue.aco-buildingdrainage.com/Home/Products/Collect/Bathroom-drainage/Bathroom-gullies/Easyflow/Gully-bodies-DN-50" (IFCTEXT)
    RSen_C_intended_use = "Entwässerungssysteme" (IFCTEXT)
    installation_manual = "http://catalogue.aco-buildingdrainage.com/Home/Products/Collect/Bathroom-drainage/Bathroom-gullies/Easyflow/Gully-bodies-DN-50" (IFCTEXT)
    instructions_for_use = "http://catalogue.aco-buildingdrainage.com/Home/Products/Collect/Bathroom-drainage/Bathroom-gullies/Easyflow/Gully-bodies-DN-50" (IFCTEXT)
  General | properties | on 1 type object
    RSen_C_code_ETIM = "EC010284" (IFCTEXT)
    RSen_C_code_manufacturer_gln = "4399901709010" (IFCTEXT)
    RSen_C_content_creator = "ACO Technology Centre Private Limited" (IFCTEXT)
    RSen_C_content_version = "1.0" (IFCTEXT)
    RSen_C_info_commercial = "http://catalogue.aco-buildingdrainage.com/Home/Products/Collect/Bathroom-drainage/Bathroom-gullies/Easyflow/Gully-bodies-DN-50" (IFCTEXT)
    RSen_C_info_technical = "http://catalogue.aco-buildingdrainage.com/Home/Products/Collect/Bathroom-drainage/Bathroom-gullies/Easyflow/Gully-bodies-DN-50" (IFCTEXT)
    RSen_C_intended_use = "Entwässerungssysteme" (IFCTEXT)
    installation_manual = "http://catalogue.aco-buildingdrainage.com/ilcatalogue/download/ZG9jdW1lbnQvZG93bmxvYWQucGRmL2RlL2sxMl9UZWNobmlzY2hlckJhZHByb3NwZWt0LUFDTy1IYXVzdGVjaG5pa19fNjcyOTgucGRm/k12_TechnischerBadprospekt-ACO-Haustechnik__67298.pdf" (IFCTEXT)
    instructions_for_use = "http://catalogue.aco-buildingdrainage.com/cz_en/Home/Products/Collect/Bathroom-drainage/Bathroom-gullies/Easyflow/Gully-bodies-DN-50" (IFCTEXT)
  General | properties | on 1 type object
    RSen_C_code_ETIM = "EC010284" (IFCTEXT)
    RSen_C_code_manufacturer_gln = "4399901709010" (IFCTEXT)
    RSen_C_content_creator = "ACO Technology Centre Private Limited" (IFCTEXT)
    RSen_C_content_version = "1.0" (IFCTEXT)
    RSen_C_info_commercial = "http://catalogue.aco-buildingdrainage.com/ilcatalogue/download/ZG9jdW1lbnQvZGF0YXNoZWV0L2VuL2RhdGFzaGVldF8yMDQwMDAwMl9TQkYtQkRfZW4ucGRm/datasheet_20400002_SBF-BD_en.pdf" (IFCTEXT)
    RSen_C_info_technical = "http://catalogue.aco-buildingdrainage.com/ilcatalogue/download/ZG9jdW1lbnQvZGF0YXNoZWV0L2VuL2RhdGFzaGVldF8yMDQwMDAwMl9TQkYtQkRfZW4ucGRm/datasheet_20400002_SBF-BD_en.pdf" (IFCTEXT)
    RSen_C_intended_use = "Entwässerungssysteme" (IFCTEXT)
    installation_manual = "http://catalogue.aco-buildingdrainage.com/ilcatalogue/download/ZG9jdW1lbnQvZG93bmxvYWQucGRmL2RlL2sxMl9UZWNobmlzY2hlckJhZHByb3NwZWt0LUFDTy1IYXVzdGVjaG5pa19fNjcyOTgucGRm/k12_TechnischerBadprospekt-ACO-Haustechnik__67298.pdf" (IFCTEXT)
    instructions_for_use = "http://catalogue.aco-buildingdrainage.com/ilcatalogue/download/ZG9jdW1lbnQvZG93bmxvYWQucGRmL2RlL0dlYnJhdWNoc2FubGVpdHVuZ19Cb2RlbmVudHdhZXNzZXJ1bmdfRWFzeWZsb3dfc2Vua3JlY2h0X182NzI1OS5wZGY=/Gebrauchsanleitung_Bodenentwaesserung_Easyflow_senkrecht__67259.pdf" (IFCTEXT)
  General: 2 more contents on 0 objects not shown
  Insulation | properties | on 1 object (1 IFCFLOWFITTING)
    Insulation Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Size = "" (IFCTEXT)
  Mechanical | properties | on 1 object (1 IFCFLOWFITTING)
    Flow Rate = "1.5 L/s" (IFCTEXT)
    Loss Method = "3bf616f9-6b98-4a21-80ff-da1120c8f6d6" (IFCTEXT)
  Phasing | properties | on 5 objects (3 IFCFLOWTERMINAL, 1 IFCFLOWCONTROLLER, 1 IFCFLOWFITTING)
    Phase Created = "New Construction" (IFCLABEL)
  Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "Anno_Level_Head_Circle: Standard" (IFCLABEL)
    Symbol at End 1 Default = TRUE (IFCBOOLEAN)
    Symbol at End 2 Default = FALSE (IFCBOOLEAN)
  Materials and Finishes | properties | on 2 objects (2 IFCFLOWTERMINAL) | on 1 type object
    RSen_C_material = "Plastic,Black" (IFCLABEL)
  Materials and Finishes | properties | on 1 object (1 IFCFLOWTERMINAL)
    RSen_C_material = "Plastic, Grey" (IFCLABEL)
  Materials and Finishes | properties | on 1 type object
    RSen_C_material = "Concrete, Lightweight, 45" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)