IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView, QuantityTakeOffAddOnView]"
Time stamp: "2017-05-26T15:58:34"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20160225_1515(x64) - Exporter 17.0.416.0 - Default UI"
Application: "Autodesk Revit 2017 (ENU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (ENU)"

People and organizations
  Person "palleri" of Organization (no name given)
  Owner history of Person "palleri" of Organization (no name given) | application "Autodesk Revit 2017 (ENU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (ENU)" | change NOCHANGE | created 1495794510 (2017-05-26T10:28:30Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 2 elements
          1 x IFCFLOWTERMINAL | type IFCWASTETERMINALTYPE "DN32" | object type "DN32" | names: "PF_ST_ShowerDrain S single connection_ACO:DN32:5995" | material: materials ("ABS, White", "Stainless Steel, Brushed Electropolished") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Constraints, Dimensions, General, Identity Data
          1 x IFCBUILDINGELEMENTPROXY | object type "Solid" | names: "ZZZ_do not use_PF_ST_grating for ShowerDrain S_ACO:Solid:6002" | material: "Stainless Steel, Brushed Electropolished" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Constraints, Dimensions, General, Identity Data

Types
  IFCWASTETERMINALTYPE "DN32" | GULLYTRAP | 1 occurrence | material: materials ("ABS, White", "Stainless Steel, Brushed Electropolished") | property sets: General, Identity Data, Materials and Finishes, Mechanical, Other | description "Drainage channel S for shower area"

Property sets
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Other | properties | on 1 object (1 IFCFLOWTERMINAL)
    Category = "Plumbing Fixtures" (IFCLABEL)
    Family = "PF_ST_ShowerDrain S single connection_ACO: DN32" (IFCLABEL)
    Family and Type = "PF_ST_ShowerDrain S single connection_ACO: DN32" (IFCLABEL)
    RSen_C_height = 85. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_length_maximal = 900. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_length_minimal = 700. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_width = 94. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_P_c01_diameter = 32. (IFCLENGTHMEASURE) [MILLI METRE]
    Type = "PF_ST_ShowerDrain S single connection_ACO: DN32" (IFCLABEL)
    Type Id = "PF_ST_ShowerDrain S single connection_ACO: DN32" (IFCLABEL)
    angle = 270. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    connector1_Z_position = 23.9 (IFCLENGTHMEASURE) [MILLI METRE]
    connector1_position = 131. (IFCLENGTHMEASURE) [MILLI METRE]
    grating_height_calculated = 22. (IFCLENGTHMEASURE) [MILLI METRE]
    length_calculated = 700. (IFCLENGTHMEASURE) [MILLI METRE]
    lookup_table_name = "showerdrain s" (IFCTEXT)
    product_index = 1 (IFCINTEGER)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Plumbing Fixtures" (IFCLABEL)
    Family = "ZZZ_do not use_PF_ST_grating for ShowerDrain S_ACO: Solid" (IFCLABEL)
    Family and Type = "ZZZ_do not use_PF_ST_grating for ShowerDrain S_ACO: Solid" (IFCLABEL)
    H = 22. (IFCLENGTHMEASURE) [MILLI METRE]
    Type = "ZZZ_do not use_PF_ST_grating for ShowerDrain S_ACO: Solid" (IFCLABEL)
    Type Id = "ZZZ_do not use_PF_ST_grating for ShowerDrain S_ACO: Solid" (IFCLABEL)
    cover_height = 28. (IFCLENGTHMEASURE) [MILLI METRE]
    cover_width = 30. (IFCLENGTHMEASURE) [MILLI METRE]
    lookup_table_name = "grating showerdrain s" (IFCTEXT)
    product_index = 1 (IFCINTEGER)
    solid = TRUE (IFCBOOLEAN)
    stripes = FALSE (IFCBOOLEAN)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Level 1" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level: Level 1" (IFCLABEL)
    Type Id = "Level: Level 1" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Plumbing Fixtures" (IFCLABEL)
    Family Name = "ZZZ_do not use_PF_ST_grating for ShowerDrain S_ACO" (IFCTEXT)
  Other | properties | on 1 type object
    Category = "Plumbing Fixtures" (IFCLABEL)
    Family Name = "PF_ST_ShowerDrain S single connection_ACO" (IFCTEXT)
  Pset_ManufacturerTypeInformation | properties | on 2 objects (1 IFCBUILDINGELEMENTPROXY, 1 IFCFLOWTERMINAL)
    Manufacturer = "ACO" (IFCLABEL)
  Pset_DistributionFlowElementCommon | properties | on 1 object (1 IFCFLOWTERMINAL)
    Reference = "DN32" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCFLOWTERMINAL)
    Host = "None" (IFCTEXT)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_length = 700. (IFCLENGTHMEASURE) [MILLI METRE]
    check_height = "Maximal height exceeded" (IFCTEXT)
    check_length = "-" (IFCTEXT)
    grating_height = 21.9999999999971 (IFCLENGTHMEASURE) [MILLI METRE]
    grating_height_check = "-" (IFCTEXT)
    grating_type = "Solid" (IFCLABEL)
    height = 163.669824613296 (IFCLENGTHMEASURE) [MILLI METRE]
    left = TRUE (IFCBOOLEAN)
    length_rounddown = TRUE (IFCBOOLEAN)
    length_roundup = FALSE (IFCBOOLEAN)
    right = FALSE (IFCBOOLEAN)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Host = "None" (IFCTEXT)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 22. (IFCLENGTHMEASURE) [MILLI METRE]
    cover_length = 700. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Dimensions | properties | on 1 object (1 IFCFLOWTERMINAL)
    Area = 0.123910818691197 (IFCAREAMEASURE) [SQUARE_METRE]
    DN = 32. (IFCLENGTHMEASURE) [MILLI METRE]
    L1 = 700. (IFCLENGTHMEASURE) [MILLI METRE]
    L2 = 760. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.000652087360770265 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    W1 = 34. (IFCLENGTHMEASURE) [MILLI METRE]
    W2 = 94. (IFCLENGTHMEASURE) [MILLI METRE]
    grating_H1 = 11. (IFCLENGTHMEASURE) [MILLI METRE]
    grating_H2 = 14. (IFCLENGTHMEASURE) [MILLI METRE]
    grating_H3 = 16. (IFCLENGTHMEASURE) [MILLI METRE]
    grating_H4 = 18. (IFCLENGTHMEASURE) [MILLI METRE]
    grating_H5 = 22. (IFCLENGTHMEASURE) [MILLI METRE]
    h_max = 85. (IFCLENGTHMEASURE) [MILLI METRE]
    h_min = 55. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 0.0799120000000037 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.000391999999999995 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  General | properties | on 1 object (1 IFCFLOWTERMINAL)
    RSen_C_code_ETIM = "EC011720" (IFCTEXT)
    RSen_C_grounding = TRUE (IFCBOOLEAN)
    RSen_S_net_mass = 2.425 (IFCREAL)
  General | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    RSen_S_net_mass = 0.968 (IFCREAL)
  General | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    RSen_C_code_ETIM = "EC011726" (IFCTEXT)
    RSen_C_code_manufacturer_gln = "4399901709010" (IFCTEXT)
    RSen_C_code_specification_URL = "" (IFCTEXT)
    RSen_C_content_creator = "Itannex bv" (IFCTEXT)
    RSen_C_content_date_changed = "" (IFCTEXT)
    RSen_C_content_version = "1.0" (IFCTEXT)
    RSen_C_info_commercial = "" (IFCTEXT)
    RSen_C_info_technical = "http://catalogue.aco-haustechnik.de/en/Home/Products/Collect/Bathroom-drainage/Channel/ACO-ShowerDrain-S/Design-gratings-made-of-ground-stainless-steel" (IFCTEXT)
    RSen_C_intended_use = "Drainage systems" (IFCTEXT)
  General | properties | on 1 type object
    RSen_C_code_manufacturer_gln = "4399901709010" (IFCTEXT)
    RSen_C_code_specification_URL = "" (IFCTEXT)
    RSen_C_content_creator = "Itannex bv" (IFCTEXT)
    RSen_C_content_date_changed = "" (IFCTEXT)
    RSen_C_content_version = "1.0" (IFCTEXT)
    RSen_C_info_commercial = "" (IFCTEXT)
    RSen_C_info_technical = "http://catalogue.aco-haustechnik.de/en/Home/Products/Collect/Bathroom-drainage/Channel/ACO-ShowerDrain-S" (IFCTEXT)
    RSen_C_intended_use = "Drainage systems" (IFCTEXT)
    installation_manual = "" (IFCTEXT)
    instructions_for_use = "http://katalog.aco-haustechnik.de/ilcatalogue/download/ZG9jdW1lbnQvZG93bmxvYWQucGRmL2RlL0lNMDAwNjI0M19fMTM4ODI2LnBkZg==/IM0006243__138826.pdf" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCFLOWTERMINAL)
    Mark = "1" (IFCTEXT)
    RSen_C_code_article = "9010.75.00" (IFCTEXT)
    RSen_C_code_gtin = "04002626503442" (IFCTEXT)
    RSen_C_description = "ACO ShowerDrain S showerdrain DN32/ 700x94/ 0,55l/s" (IFCTEXT)
    RSen_C_type_comments = "Fl. hori/ WS25/ V2A/ Kst" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Mark = "2" (IFCTEXT)
    RSen_C_code_article = "9010.75.50" (IFCTEXT)
    RSen_C_code_gtin = "04002626503626" (IFCTEXT)
    RSen_C_description = "ACO ShowerDrain S Rost/grating 700/ Plate/ V2A/ K3" (IFCTEXT)
    RSen_C_type_comments = "-" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "Solid" (IFCTEXT)
    LOD = "LOD 400" (IFCTEXT)
    Manufacturer = "ACO" (IFCTEXT)
    Model = "ACO grating for ShowerDrain S" (IFCTEXT)
    OmniClass Number = "23.70.50.21.24" (IFCTEXT)
    OmniClass Title = "Waste Water Drains" (IFCTEXT)
    Type Name = "Solid" (IFCTEXT)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "Drainage channel S for shower area" (IFCTEXT)
    LOD = "LOD 400" (IFCTEXT)
    Manufacturer = "ACO" (IFCTEXT)
    Model = "ACO ShowerDrain S" (IFCTEXT)
    OmniClass Number = "23.70.50.21.24" (IFCTEXT)
    OmniClass Title = "Waste Water Drains" (IFCTEXT)
    Type Comments = "Tested according EN 1253-1 for load capacity and flow capacity" (IFCTEXT)
    Type Name = "DN32" (IFCTEXT)
  Mechanical | properties | on 1 object (1 IFCFLOWTERMINAL)
    RSen_P_c01_flow = 0.0194230666968187 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Sanitary" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 1 type object
    WFU = 2. (IFCREAL)
  Phasing | properties | on 2 objects (1 IFCBUILDINGELEMENTPROXY, 1 IFCFLOWTERMINAL)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Solid" (IFCIDENTIFIER)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Materials and Finishes | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    RSen_C_material = "Stainless Steel, Brushed Electropolished" (IFCLABEL)
  Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)